Cengiz Alaettinoglu, IETF, Montreal, June 1996 10 of 10

Peering via 3rd Party

as-in: from AS1 7.7.7.1 7.7.7.2 via AS3 7.7.7.3 accept AS1

GONE!!!

Cengiz Alaettinoglu, IETF, Montreal, June 1996 9 of 10

        More Specific Operators

128.9.0.0/16+ inclusive more specifics
128.9.0.0/16* exclusive more specifics
128.9.0.0/16/25 length 25 more specifics
128.9.0.0/16/25-32 length 25-32 more specifics

128.9.0.0/16^+ inclusive
128.9.0.0/16^- exclusive
128.9.0.0/16^25 length 25
128.9.0.0/16^25-32 length 25-32

Need better suggestions!

Cengiz Alaettinoglu, IETF, Montreal, June 1996 8 of 10

Peering Specification

<local-router> and <peer-router> are router names:

Before: as-in: from AS1 7.7.7.1 7.7.7.2

                  accept AS1

Now: as-in: from AS1 rtr.foo.net rtr.bar.net

                  accept AS1

* form is removed

Before: as-in: from AS1 * * accept AS1 Now: as-in: from AS1 accept AS1 Before: as-in: from AS1 7.7.7.1 * accept AS1 Now: as-in: from AS1 rtr.foo.net accept AS1

Cengiz Alaettinoglu, IETF, Montreal, June 1996 7 of 10

Policy Expr essions

The following keywords are no longer optional:

from, action, accept, to, announce

 aut-num: AS1
 as-in: from AS2 action pref = 1 accept AS2

 as-in: AS2 10 AS2

Cengiz Alaettinoglu, IETF, Montreal, June 1996 6 of 10

Route Class

            route: 128.7.0.0/16
            origin: AS1
            aggregate-by: ATOMIC ANY
            inject-at: foo.bar.net
            export-components: { 128.7.9.0/24 }

inject-at is a list of router names

export-components replaces supress-components

Components are exported to all neighboring ASes Before: exported to allpeer routers of injecting routers

Cengiz Alaettinoglu, IETF, Montreal, June 1996 5 of 10

Maintainer Class

Maintainer names start with “MAINT-”

MAINT-FOO, maint-as226

Cengiz Alaettinoglu, IETF, Montreal, June 1996 4 of 10

Object Repr esentation

Lines of attribute-value pairs ends at a blank line attribute name at column 0 followed by “:” then value lines continued by placing space or tab at column 0 order of attribute-value pairs is significant

aut-num: AS1
as-in:   from AS2
         accept AS2
as-out:  to AS2 announce ANY

route: 128.9.0.0/16

Cengiz Alaettinoglu, IETF, Montreal, June 1996 3 of 10

AS Number

AS0, AS226, AS3561

IP Addr ess

128.9.128.10

Addr ess Prefix

128.9.0.0/16, 0.0.0.0/0 0/0, 128.8/16

Date

19/08/1966 190866
19660819 ???

Cengiz Alaettinoglu, IETF, Montreal, June 1996 2 of 10

RPSL Names

Composed of a-z, 0-9, “_”, “-” Starts with a-z Ends with a-z, 0-9 Case insensitive

as-foo as-226-customers cENgiZ cengiz

Reserved words:

from to announce accept action
any as-irr rs-irr atomic
and or not

Cengiz Alaettinoglu, IETF, Montreal, June 1996 1 of 10

Changes to RPSL Specification

Cengiz Alaettinoglu

<cengiz@isi.edu>

Slides: ftp://ftp.isi.edu/rps/montreal-ietf